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LBTD216G  
16-port 10/100/1000BASE-TX +2G SFP Industrial Ethernet Switch  
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· 16-Port 10/100/1000Base-Tx RJ-45 with auto  negotiation and auto-MDI/MDI-X function
· 2-Port SFP uplink
 Industrial conformance
· 12V to 52V DC, redundant power input
· -40℃ to 80℃ operating temperature
· IP40 aluminum housing
· Supports Air discharge: ±12kV
· Contact discharge: ±8kV
· Free Fall, Shock and Vibration Stability
· DIN-rail hardware design


Slim Type with more Practicability and Convenience
[bookmark: _GoBack]LBTD216G an hardened 16-port Industrial Ethernet Switch, provides non-blocking wire-speed performance in harsh industrial environment. It provides 16-port 10/100/1000BASE-TX RJ45 copper interfaces +2 Port 10/100/1000 SFP delivered in an IP40 rugged, strong case with redundant power system. Its slim case is suitable for such applications as surveillance system deployments, control management and wireless service in climatically demanding environments with wide temperature range from -40℃ to 80℃.

The LBTD216G series provides the flexibility to all kinds of 10/100Mbps Ethernet Media on RJ-45 port and performs highly stable fiber performance.

The LBTD216G series is packaged in a compact IP40 case that allows either DIN rail or panel mounting to have efficient usage of cabinet space. It provides an integrated power supply with a wide range of voltages for worldwide operation. It also offers dual-redundant, reversible polarity 12V DC to 52V DC power supply inputs for high availability applications requiring dual or backup power inputs.




Specifications:
	Model No.
	LBTD216G

	10/100/1000BASE-TX Port
	16 port RJ-45 auto-MDI / MDI-X 
2 port SFP

	
Performance Specification
	Bandwidth: 56Gbps 
Packet Buffer Memory:4.1Mbit
Packet Forwarding Rate: 42Mpps
MAC Address Table: 8K

	Installation
	DIN rail 

	Maximum Frame Size
	9000bytes packet size

	Flow Control
	Back pressure for half duplex, IEEE 802.3x pause frame for full duplex

	Enclosure
	IP40 aluminum housing

	
LED Indicator
	Power: Red
Ethernet: Yellow 
POE: Green 
P.S LBTD216G not with PoE function

	Power Input
	12 to 52V DC redundant power 

	Power Consumption
	10 watts

	Surge protection
	±4KV 

	
Network Protocols
	IEEE802.3 10BASE-T; 
IEEE802.3i 10Base-T; 
IEEE802.3u;100Base-TX/FX; 
IEEE802.3ab 1000Base-T;  
IEEE802.3z 1000Base-X; 
IEEE802.3x;

	Network cables
	10BASE-T: Cat3,4,5 UTP(≤100 meter)     
100BASE-TX: Cat5 or later UTP(≤10meter)
1000BASE-TX: Cat6 or later UTP(≤100 meter)

	

Industry Standard
	IEC 61000-4-4 (EFT), Level 3
IEC 61000-4-5 (Surge), Level 3
Shock: IEC 60068-2-27
Free fall: IEC 60068-2-32
Vibration: IEC 60068-2-6

	MTBF
	>300,000hours

	Certification
	CE FCC Rohs compliance

	Dimensions (W x D x H)
	175.6 x 135 x 45.5 mm

	Weight
	Product Weight: 0.9KGS
Packing Weight: 1.0KGS

	Working Environment

	Working temperature: -40～80℃ ;  
Storage temperature: -40～80℃
Relative Humidity: 5%~95 %( no condensation)

	Warranty 
	1-year replacement with new item; 3-years for main parts.  















Dimensions
[image: ]

image2.png




image3.png
— 135] —

b

s

B mm




image1.png
(EFCE@ @ @ G




