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LBTD48G-SFP 
8-port 10/100/1000BASE-TX+4-port SFP Industrial Ethernet Switch  
     [image: ] [bookmark: _Hlk72766732]Interface
· 8-Port 10/100/1000Base-Tx RJ-45 with auto  negotiation and auto-MDI/ MDI-X function
· 4-Port SFP 

 Industrial conformance
· 12V to 52V DC, redundant power input
· -40℃ to 80℃ operating temperature
· IP40 aluminum housing
· Supports 6KV DC Ethernet ESD protection
· Supports 6KV DC EFT protection for power line
· Free Fall, Shock and Vibration Stability
· DIN-rail design

 
[bookmark: _GoBack]LBTD48G-SFP an hardened 12-port Industrial Ethernet Switch, provides non-blocking wire-speed performance in harsh industrial environment. It also provides 8-port 10/100/1000BASE-TX RJ45 +4-port SFP delivered in an IP40 rugged, strong case with redundant power system. Its slim case is suitable for such applications as surveillance system deployments, control management and wireless service in climatically demanding environments with wide temperature range from -40℃ to 80℃.

The LBTD48G-SFP provides the flexibility to all kinds of 10/100/1000Mbps Ethernet Media on RJ-45 port and performs highly stable fiber performance.



Specifications:ROBOT
ROBOT

	Model No.
	LBTD48G-SFP

	10/100/1000Base-TX Port
	8 port RJ-45 auto-MDI / MDI-X

	1000Base-FX Port
	4 port SFP

	
Performance Specification
	Bandwidth: 52Gbps
Packet Buffer Memory:2Mbit
Packet Forwarding Rate:41.7Mpps
MAC Address Table: 8K

	Installation
	DIN rail

	Maximum Frame Size
	9000bytes packet size

	Flow Control
	Back pressure for half duplex, IEEE 802.3x pause frame for full duplex

	Enclosure
	IP40 aluminum housing

	
LED Indicator
	Power: Red
Fiber: Green
Ethernet: Yellow 

	Power Input
	12 to 52V DC redundant power 

	Power Consumption
	< 10 watts

	Surge protection
	±4KV 

	
Network Protocols
	IEEE802.3 10BASE-T; 
IEEE802.3i 10Base-T; 
IEEE802.3u;100Base-TX/FX; 
IEEE802.3ab 1000Base-T;  
IEEE802.3z 1000Base-X; 
IEEE802.3x;

	Network cables
	10BASE-T: Cat3,4,5 UTP(≤100 meter)     
100BASE-TX: Cat5 or later UTP(≤100 meter)
1000BASE-TX: Cat6 or later UTP(≤100 meter)

	

Industry Standard
	FCC CFR47 Part 15,EN55032, Class A 
IEC61000-4-2 (ESD): ±8kV (contact), ±12kV (air)
IEC61000-4-3 (RS): 10V/m (80~1000MHz)
IEC61000-4-5 (Surge): Power Port: ±2kV/DM, ±4kV/CM; Data Port: ±2kV
IEC61000-4-6 (CS): 3V (10kHz-150kHz); 10V (150kHz-80MHz)
IEC61000-4-16 (Common mode conduction): 30V (cont.), 300V (1s)

	MTBF
	300,000hours

	Dimensions (W x D x H)
	143.7 x 125 x 47.7mm

	Weight
	Product Weight: 0.64KG
Packing Weight: 0.74KG

	Working Environment

	Working temperature: -40～80℃ ;  
Storage temperature: -40～80℃
Relative Humidity: 5%~95 %( no condensation)
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