

                                                                      [image: ]
[bookmark: _GoBack]LBT24GSP-M-SFP   

4-port 10//100/1000BASE-TX+2G SFP Managed Industrial Switch  
    [image: E:\YH产品资料202006\VTS网管\入地2光4电\IMG_0478.JPGIMG_0478][bookmark: _Hlk72766732]Interface
· 4-port 10/100Base-Tx RJ-45 with auto negotiation and auto-MDI/ MDI-X  function
· 2-port gigabit SFP 

 Industrial conformance
· 12V to 52V DC, redundant power input
· -40℃ to 80℃ operating temperature
· IP40 aluminum housing 
· Supports 6KV DC Ethernet ESD protection
· Supports 6KV DC EFT protection for power line
· Free Fall, Shock and Vibration Stability
· DIN-rail and wall-mountable hardware design

Slim Type with more Practicability and Convenience
LBT24GS-M-SFP an hardened 6-port Industrial Ethernet Switch, provides non-blocking wire-speed performance in harsh industrial environment. It also provides 4-port 10/100BASE-TX RJ45 +2G SFP delivered in an IP40 rugged, strong case with redundant power system. Its slim case is suitable for such applications as surveillance system deployments, control management and wireless service in climatically demanding environments with wide temperature range from -40℃ to 80℃.

The LBT24GS-M-SFP provides the flexibility to all kinds of 10/1000Mbps Ethernet Media on RJ-45 port and performs highly stable fiber performance.
L2 management     
· Support STP/RSTP/MSTP 
· Web management, CLI
· IGMP snooping, QOS,VLAN,SNMP


The LBT24GS-M-SFP is packaged in a compact IP40 case that allows either DIN rail or panel mounting to have efficient usage of cabinet space. It provides an integrated power supply with a wide range of voltages for worldwide operation. It also offers dual-redundant, reversible polarity 12V DC to 52V DC power supply inputs for high availability applications requiring dual or backup power inputs.

Specifications:ROBOT
ROBOT

	Model No.
	LBT24GS-M-SFP

	1000Base-TX Port
	4 port RJ-45 auto-MDI / MDI-X

	1000Base-FX Port
	2G SFP Slot

	
Performance Specification
	Bandwidth (switch capacity): 38Gbps 
Packet Buffer Memory: 12Mbit
Packet Forwarding Rate: 28.3Mpps
MAC Address Table: 8K

	Installation
	DIN rail

	Maximum Frame Size
	10240bytes 

	Flow Control
	Back pressure for half duplex, IEEE 802.3x pause frame for full duplex

	Enclosure
	IP40 slim type metal case

	
LED Indicator
	Power: Red
Fiber: Link 2(Green)
Ethernet: Yellow 

	Power Input
	12 to 52V DC redundant power 

	Power Consumption
	3 watts 

	Surge Protection
	± 4KV

	
Network Protocols
	IEEE802.3 10BASE-T; 
IEEE802.3i 10Base-T; 
IEEE802.3u;100Base-TX/FX; 
IEEE802.3ab 1000Base-T;  
IEEE802.3z 1000Base-X; 
IEEE802.3x;

	Network cables
	10BASE-T: Cat3,4,5 UTP(≤100 meter)     
100BASE-TX: Cat5 or later UTP(≤10meter)
1000BASE-TX: Cat6 or later UTP(≤100 meter)

	

Industry Standard
	FCC CFR47 Part 15,EN55022/CISPR22, Class A 
IEC61000-4-2 (ESD): ±8kV (contact), ±12kV (air)
IEC61000-4-3 (RS): 10V/m (80~1000MHz)
IEC61000-4-4 (EFT): Power Port: ±4kV; Data Port: ±2kV
IEC61000-4-5 (Surge): Power Port: ±2kV/DM, ±4kV/CM; Data Port: ±2kV
IEC61000-4-6 (CS): 3V (10kHz-150kHz); 10V (150kHz-80MHz)
IEC61000-4-16 (Common mode conduction): 30V (cont.), 300V (1s)

	Certificate
	CE FCC Rohs compliance

	MTBF
	>300,000hours

	Dimensions (W x D x H)
	143.7 x 103 x 44.2 mm   

	Weight
	Product Weight: 0.36KG
Packing Weight: 0.46KG

	Working Environment

	Working temperature: -40～80℃ ;  
Storage temperature: -40～80℃
Relative Humidity: 5%~95 %( no condensation)

	Warranty 
	1-year replacement with new item; 3-years for main parts.  













Dimensions
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Ordering Information
	LBT24GS-M-SFP
	4-port 10/100/100BASE-TX+2G SFP Managed Industrial Switch
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