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LBT424GS-M-SFP   
24-port 10//100/1000BASE-TX+4G combo Managed Industrial Switch  
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· 24-port 10/100/1000Base-Tx RJ-45 with auto negotiation and auto-MDI/ MDI-X  function
· 4G combo (4G RJ45 or 4G SFP)

 Industrial conformance
· 36V to 72V DC,AC110-240V redundant power input
· - 40℃ to 85℃ operating temperature
· IP40 aluminum housing 
· Supports 6KV DC Ethernet ESD protection
· Supports 6KV DC EFT protection for power line
· Free Fall, Shock and Vibration Stability
· Rak-mountable hardware design

 
LBT424GS-M-SFP an hardened 32-port Industrial Ethernet Switch, provides non-blocking wire-speed performance in harsh industrial environment. It also provides 24-port 10/100/1000BASE-TX RJ45 +4G combo delivered in an IP40 rugged, strong case with redundant power system. It’s suitable for such applications as surveillance system deployments, control management and wireless service in climatically demanding environments with wide temperature range from -40℃ to 85℃.

The LBT424GS-M-SFP provides the flexibility to all kinds of 10/100/1000Mbps Ethernet Media on RJ-45 port and performs highly stable fiber performance.

The LBT424GS-M-SFP is packaged in a compact IP40 case that allows bracket mounting to cabinet . It supplies dual power supply: DC36~72V and AC110-240V
Specifications:ROBOT
ROBOT

	Model No.
	LBT424GS-M-SFP

	1000Base-TX Port
	24G port RJ-45 auto-MDI / MDI-X

	Uplink Port
	4G combo (either 4G RJ45 or 4G SFP)

	
Performance Specification
	Bandwidth: 256Gbps 
Packet Buffer Memory: 16Mbit
Packet Forwarding Rate: 131Mpps
MAC Address Table: 16K

	Installation
	Rak mounted

	Maximum Frame Size
	10240bytes packet size

	Flow Control
	Back pressure for half duplex, IEEE 802.3x pause frame for full duplex

	Enclosure
	[bookmark: _Hlk74143321]IP40 Aluminum housing 

	
LED Indicator
	Power: Red
Fiber: Link 2(Green)
Ethernet: Yellow 

	Dual Power Input
	36 to 72V DC and AC110-240V

	Power Consumption
	< 10W

	Surge protection
	 ± 4KV

	
Network Protocols
	IEEE802.3 10BASE-T; 
IEEE802.3i 10Base-T; 
IEEE802.3u;100Base-TX/FX; 
IEEE802.3ab 1000Base-T;  
IEEE802.3z 1000Base-X; 
IEEE802.3x;

	Network cables
	10BASE-T: Cat3,4,5 UTP(≤100 meter)     
100BASE-TX: Cat5 or later UTP(≤100meter)
1000BASE-TX: Cat6 or later UTP(≤100 meter)

	

Industry Standard
	FCC CFR47 Part 15,EN55022/CISPR22, Class A 
IEC61000-4-2 (ESD): ±8kV (contact), ±12kV (air)
IEC61000-4-3 (RS): 10V/m (80~1000MHz)
IEC61000-4-4 (EFT): Power Port: ±4kV; Data Port: ±2kV
IEC61000-4-5 (Surge): Power Port: ±2kV/DM, ±4kV/CM; Data Port: ±2kV
IEC61000-4-6 (CS): 3V (10kHz-150kHz); 10V (150kHz-80MHz)
IEC61000-4-16 (Common mode conduction): 30V (cont.), 300V (1s)

	Certification
	CE FCC Rohs compliance

	MTBF
	>300,000hours

	Dimensions (W x D x H)
	442×325×44mm

	Weight
	Product Weight: 3.26KG
Packing Weight: 4KG

	Working Environment

	Working temperature: -40～85℃ ;  
Storage temperature: -40～85℃
Relative Humidity: 5%~95 %( no condensation)

	Warranty 
	1-year replacement with new item; 3-years for main parts.  



Software:
	Port Features 
	IEEE 802.3x Flow control

	
	Interface counters

	
	Storm Control

	Link Aggregation 
	Static Aggregation

	
	Dynamic Aggregation, LACP

	
	Supports up to 8 aggregation groups, each group up to 8 ports
Support source MAC, destination MAC, source destination MAC, source IP, destination IP, source destination IP routing strategy

	MAC Table Management
	Support

	Forwarding mode
	Support IVL forwarding mode

	Static MAC Address
	Support

	MAC Address Binding
	Support

	MAC Address Filtering
	Support

	Mirror 
	Port-based Mirror

	Spanning Tree 
	IEEE802.1d STP

	
	IEEE802.1w RSTP

	
	IEEE802.1s MSTP

	ERPS (G.8032) 
	Single Ring, Sub-Ring, Multi-Ring

	
	Load balance

	
	Recovery Time < 50ms

	GVRP 
	Supported

	QINQ 
	VLAN-based QinQ

	LLDP 
	LLDP

	
	LLDP-MED

	Loop Protection 
	Supported

	VLAN 
	4094 VLAN

	
	Port-based VLAN

	
	GVRP

	Protocol VLAN 
	MAC-based VLAN

	
	IP Subnet-based VLAN

	Voice VLAN 
	Static entry

	
	LLDP-MED

	Port Isolate 
	Support

	IGMP 
	Snooping IGMP V1 Snooping

	
	IGMP V2 Snooping

	
	IGMP V3 Snooping

	
	Source Port Check

	
	IGMP Fast Leave

	
	IGMP Filter

	MLD Snooping 
	MLD V1 Snooping

	
	MLD V2 Snooping

	
	Source Port Check

	
	MLD Fast Leave

	
	MLD Filter

	Security
	

	ACL 
	ACL (IP Standard ACL), IPv4/IPv6

	
	MAC extend ACL

	
	IP extend ACL

	
	L2, L3, L4 fields match

	
	log, redirection, mirroring, speed limit

	QoS 
	QoS Class, Remarking

	
	SP, WRR queue scheduling

	
	Ingress port-based rate-limit

	
	Ingress priority-based rate-limit

	
	Egress port-based rate-limit

	
	Egress queue-based rate-limit

	
	Policy-based QoS

	
	Storm Control

	
	8 queues per port

	Dot1x 
	Port Access Control

	
	User Access Control

	
	MAC-address Access Control

	AAA
	Support 802.1x

	
	Support RADIUS

	
	Supports authentication, authorization, and accounting through RADIUS server

	Management
	

	User management 
	Password protection

	SNMP 
	SNMP V1/V2c/V3

	RMON 
	Statistics Group

	
	History Group

	
	Alarm Group

	
	Events Group

	Web management 
	HTTP V1.1, HTTPS

	Firmware Upgrade 
	Reversion Upgrade

	IPv4/IPv6 
	Support

	CLI 
	Support

	Syslog/Debug 
	Support

	Diagnosis 
	Ping (IPv4), ping (IPv6)

	
	Trace route(IPv4)

	
	Trace route(IPv6)

	Management
	

	NTP 
	NTP Client

	DHCP 
	DHCPv4 Client, DHCPv6 Client

	DHCP Snooping 
	DHCP snooping table

	
	Trust Port

	IPv6 DHCP-Guard
	Support

	Telnet 
	Telnet Server

	TFTP 
	TFTP Client

	SSH 
	SSH Server





Dimensions
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