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Rack mounted Aluminum Industrial SwitchProduct features:
● Data control: Supports 802.3x full-duplex flow control and
network storm suppression 
● Redundant network: supports STP, RSTP, MSTP and ERPS 
● Redundancy backup: supports the virtual route redundancy protocol VRRP 
● Multicast management: Support IGMP Snooping V1, V2, and V3 
● VLAN: supports IEEE 802.1Q vlans to effectively isolate broadcast domains 
Link aggregation: Support static/dynamic link aggregation, provide perfect bandwidth utilization 
● QOS: Support COS\DSCP, 4 queues, support WRR\SP scheduling mode 
● Security management: Security management: supports ACL and 802.1x 
● Management: Supports WEB, CLI, and SNMP management 
Monitoring and maintenance: Support port mirroring, interface status monitoring, log management




[bookmark: _GoBack]LBT424GST4-M-SFP switch is a high performance 24 Port gigabit + 10G SFP+ L3 core switch. It provides Static routing and dynamic routing with advanced hardware processing capacity. The machine adopts modular design, which supports up to 4 Port 10G SFP+, and retains the expansion ability to further support 10GE when realizing gigabit convergence or access. It supports IPv4/IPv6 hardware double stack and line speed forwarding, so that customers can easily cope with the coming IPv6 era, which provides high capacity exchange capacity. LBT424GST4-M-SFP switch has the operating temperature of -40℃ ~ 80℃, has the super firmness to adapt to all kinds of harsh environment, can also be very convenient to install in the machine room cabinet. The rack-mounted characteristics and wide temperature operation make the switch a plug and play industrial-grade device, providing a reliable and convenient solution for users to network their Ethernet devices.
 

Strong processing ability
LBT424GST4-M-SFP switch is based on the powerful and stable
processing power of VCore-III MIPS-based CPU
LBT424GST4-M-SFP provides up to 1.2Tbps of switching capacity
port full speed filtering and forwarding 406Mpps
To ensure that the trunk network of large traffic data without blocking
Forwarding.






Specifications:ROBOT
ROBOT

	Model No.
	LBT424GST4-M-SFP

	Interface
	24-Port 10/100/1000Mbps RJ45
4-Port 10G SFP+ (compatible with 1000M/2500M/10000M)
1-Port console

	
Performance Specification
	Bandwidth(switch capacity): 1.2Tbps
Packet Buffer Memory:32Mbit
Packet Forwarding Rate: 406Mpps
MAC Address Table: 32K

	Installation
	Bracket mounted

	Flow Control
	Back pressure for half duplex, IEEE 802.3x pause frame for full duplex

	Enclosure
	IP40 Aluminum housing

	
LED Indicator
	POWER: Red
RUN: Green
Fiber: X1~X4(Green)
Ethernet: Yellow 

	Power Input
	AC110-240V

	Power Consumption
	< 30watts

	Surge protection
	±4KV 

	
Network Protocols
	IEEE 802.3ad, link aggregation protocols
IEEE802.3 10BASE-T; 
IEEE802.3i 10Base-T; 
IEEE802.3u;100Base-TX/FX; 
IEEE802.3ab 1000Base-T;  
IEEE802.3z 1000Base-X; 
IEEE 802.3ae,10G
IEEE 802.3x, Full duplex Ethernet data link Laminar flow control
IEEE 802.3az,EEE high efficient ethernet

	Network cables
	10BASE-T: Cat3,4,5 UTP(≤100 meter)     
100BASE-TX: Cat5 or later UTP(≤100meter)
1000BASE-TX: Cat6 or later UTP(≤100 meter)

	

Industry Standard
(EMC 4)
	FCC CFR47 Part 15,EN55032 
IEC61000-4-2 (ESD): ±8kV (contact), ±12kV (air)
IEC61000-4-3 (RS): 10V/m (80~1000MHz)
IEC61000-4-4 (EFT): Power Port: ±4kV; Data Port: ±2kV
IEC61000-4-5 (Surge): Power Port: ±2kV/DM, ±4kV/CM; Data Port: ±2kV
IEC61000-4-6 (CS): 3V (10kHz-150kHz); 10V (150kHz-80MHz)
IEC61000-4-16 (Common mode conduction): 30V (cont.), 300V (1s)

	MTBF
	300,000hours

	Dimensions (W x D x H)
	442x194x44mm

	Weight
	Product Weight: 4KGS    
Packing Weight: 4.6KGS

	Working Environment

	Working temperature: -40～80℃ ;  
Storage temperature: -40～80℃
Relative Humidity: 5%~95 %( no condensation)



Management features:
	
Interface
	IEEE802.3X (Full-duplex), Port temperature protection setting
Port green Ethernet Energy-saving setting Broadcast storm control based 
on port speed. The speed limit of the message flow in the access port.
The minimum particle size is 64Kbps.

	Layer 3 Features
	L3 network management, IPV4/IPV6 management L3 soft routing forwarding, 
Static route, Default route @ 128 pcs, APR@1024pcs

	

VLAN
	4K VLAN based on port, IEEE802.1q 
VLAN based on the protocol
VLAN based on MAC
VLAN based on IP
Voice VLAN, QinQ configuration
Port configuration of Access, Trunk, Hybrid

	Port Aggregation
	LACP, Static aggregation
Max 14 aggregation groups and 16 ports per group.

	Spanning Tree
	STP (IEEE802.1d), RSTP (IEEE802.1w), MSTP (IEEE802.1s)

	Industrial Ring
Network Protocol
	G.8032 (ERPS), Recovery time less than 20ms
250 Ring at most, Max 250 devices per ring. Multicast

	Multicast
	MLD Snooping v1/v2,Multicast VLAN Registration (MVR)
IGMP Snooping v1/v2, Max 1024 multicast groups, Fast log out

	Port Mirroring
	Bidirectional data mirroring based on port

	
QoS
	SP（Strict Priorty）
WFQ (Weighted Fair Queuing)
WRR (Weighted Round Robin)
Random Early Detect (RED)
WeightedRandomEarlyDetection (WRED)
Head Of Line
Best-Effort Service
First come first served
802.1p
Cos/Tos，QOS
Differentiated Service

	
ACL
	Port-based Issuing ACL,ACL based on port and VLAN
L2 to L4 packet filtering, matching first 80bytes message. 
Provide ACL based on MAC, Destination MAC address, IP Source, 
Destination IP, IP Protocol Type, TCP/UDP Port, TCP/UDP Port Range, 
and VLAN, etc.

	

Security
	Support IP ACL，MAC ACL，Vlan ACL,support ACL based on L3 L4
IP+MAC Port binding
Support IP Source Guard, RP Detection
Support IEEE 802.1x port verification, support Radius

	DHCP
	DHCP Client, DHCP Snooping, DHCP Server, DHCP Relay

	
IP routing
	Supports port-based input/output bandwidth management. 
Supports static routes. IPV6
Supports the virtual route redundancy protocol VRRP. 
Dynamic routes such as RIP, RIPng, OSPF, and OSPFv3 are supported.

	
System maintenance
	Supports configuration file uploading and downloading. Upload the upgrade package. 
Supports factory restore on WEB, Supports the system log function. 
Support  Ping 、tracert、cable detection and other diagnostic functions.
Supports WEB management (HTTP and HTTPS). 
Supports CLI management. Supports Telnet remote management. 
Supports SSH 2.0. Supports SNMP network management. 
Support RMON; Supports NTP clients. Support PTP（1588v2）
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