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Product Overview:
T300-FAP818V3 is a high-performance, high-speed indoor Wi-Fi 6 (AX3000) wall-plate access point. It offers dual-band wireless service on 2.4GHz and 5.8GHz, providing a cleaner wireless environment and more stable wireless access. 
Key Features:

Supports concurrent dual-band operation on 2.4GHz (574Mbps) and 5GHz (2402Mbps), with a maximum wireless throughput of nearly 3Gbps.

The heatsink features a special surface coating treatment for improved heat dissipation. 

Supports IEEE 802.3af standard 48V PoE power supply. 

Supports hardware watchdog function, automatically recovering abnormal devices for maintenance-free operation.

Supports interchangeable covers in multiple colors.

Hardware:
	Model
	T300-FAP818V3

	CPU 
	MT7981B + MT7976CN + RTL8211FS

	Flash
	16MB

	DDR3L
	256MB

	2.4G frequency
	2.4GHz ~ 2.484GHz

	2.4G WIFI protocol
	802.11 b / g / n / ax

	5G frequency
	5.150GHz～5.850GHz

	5G WIFI protocol
	802.11 a / n / ac / ax

	Antenna
	2 built-in dual-band onboard omnidirectional antennas, Antenna Gain: 1.7dBi

	Max rate
	2.4GHz provides up to 574Mbps access rate, 5GHz provides up to 2402Mbps access rate.

	2.4GHz tx power
	802.11b
	11M
	23±2dBm
	1M
	23±2dBm

	
	802.11g
	54M
	20±2dBm
	6M
	22±2dBm

	
	802.11n HT20
	MCS7
	18.5±2dBm
	MCS0
	20.5±2dBm

	
	802.11n HT40
	MCS7
	18.5±2dBm
	MCS0
	20.5±2dBm

	
	802.11ax HT20
	MCS11
	17±2dBm
	MCS0
	20.5±2dBm

	
	802.11ax HT40
	MCS11
	17±2dBm
	MCS0
	20.5±2dBm

	5GHz tx power
	802.11a
	54M
	19±2dBm
	6M
	21.5±2dBm

	
	802.11n HT20
	MCS7
	18±2dBm
	MCS0
	20±2dBm

	
	802.11n HT40
	MCS7
	18±2dBm
	MCS0
	20±2dBm

	
	802.11ac HT20
	MCS8
	17.5±2dBm
	MCS0
	20±2dBm

	
	802.11ac HT40
	MCS9
	17.5±2dBm
	MCS0
	20±2dBm

	
	802.11ac HT80
	MCS9
	17±2dBm
	MCS0
	19.5±2dBm

	
	802.11ax HT20
	MCS11
	16.5±2dBm
	MCS0
	20±2dBm

	
	802.11ax HT40
	MCS11
	16.5±2dBm
	MCS0
	20±2dBm

	
	802.11ax HT80
	MCS11
	16±2dBm
	MCS0
	19.5±2dBm

	
	802.11ax HT160
	MCS11
	14.5±2dBm
	MCS0
	18±2dBm

	2.4GHz Rx sensitivity
	802.11b
	11M
	-81dBm
	1M
	-90dBm

	
	802.11g
	54M
	-70dBm
	6M
	-87dBm

	
	802.11n HT20
	MCS7
	-69dBm
	MCS0
	-87dBm

	
	802.11n HT40
	MCS7
	-66dBm
	MCS0
	-84dBm

	
	802.11ax HT20
	MCS11
	-57dBm
	MCS0
	-87dBm

	
	802.11ax HT40
	MCS11
	-54dBm
	MCS0
	-84dBm

	5GHz Rx sensitivity
	802.11a
	54M
	-70dBm
	6M
	-87dBm

	
	802.11n HT20
	MCS7
	-69dBm
	MCS0 
	-87dBm

	
	802.11n HT40
	MCS7
	-66dBm
	MCS0 
	-84dBm

	
	802.11ac HT20
	MCS8
	-64dBm
	MCS0 
	-87dBm

	
	802.11ac HT40
	MCS9
	-59dBm
	MCS0
	-84dBm

	
	802.11ac HT80
	MCS9
	-56dBm
	MCS0
	-80dBm

	
	802.11ax HT20
	MCS11
	-57dBm
	MCS0
	-87dBm

	
	802.11ax HT40
	MCS11
	-54dBm
	MCS0
	-84dBm

	
	802.11ax HT80
	MCS11
	-51dBm
	MCS0
	-81dBm

	
	802.11ax HT160
	MCS11
	-48dBm
	MCS0
	-78dBm

	2.4GHz EVM
	802.11b: ≤-10 dB；802.11g: ≤-25 dB；802.11n: ≤-28dB；802.11ax: ≤-35 dB

	5GHz EVM
	802.11a: ≤-25 dB ；802.11n: ≤-28 dB ；802.11ac: ≤-32 dB;  802.11ax: ≤-35 dB

	ppm
	±20ppm

	WAN
	1 x 10/100/1000Mbps Auto-Negotiation RJ45 WAN port, supporting 48V PoE power supply

	LAN
	1 x 10/100/1000Mbps Auto-Negotiation RJ45 LAN port

	Button
	Reset button (press and hold for 6-10 seconds to restore to factory default settings)

	LED
	Built-in hidden tri-color LED (Red, Green, Blue) on the middle frame. 

Solid red on power-up. After system startup and any Wi-Fi is enabled, the red light turns off and the green light turns solid. 

In AC management mode: When the AP loses connection with the AC, the red and green lights turn off, and the blue light turns solid. 

(3) When the "Find AP" function is used, the red and green lights turn off, and the blue light flashes quickly (once per second).

	Power supply
	PoE 802.3af

	Power consumption
	<12W

	Size
	86mm × 86mm × 38.8mm (external height is 8.5mm)

	Weight
	0.15kg

	Environment
	Operating temperature-10°C to 40°C；Storage temperature: -40°C to 70°C；humidity：5％～95％（No condensation）

	ESD
	Air:±8K, Touch:±6K

	Electrical Surge
	Common Mode: 2K, Differential Mode: 1K


Firmware:
	Dashboard
	Operating Mode: Fat AP mode and Thin AP mode

Wireless AP download rate, wireless AP upload rate, uptime

Device information, device description, LAN information, WIFI information

	Supported Modes
	Gateway Mode: Connects to WAN via static IP, DHCP, or PPPoE.

AP Mode: Provides wireless coverage, connecting to an upstream router via Ethernet.

	Wireless Features
	SSID Broadcast

Number of SSIDs: 4 (2.4GHz) + 4 (5GHz)

SSID Hiding

Wireless Encryption: OPEN, WPA/WPA2PSK-TKIP/AES, WPA3-SAE

Wireless MAC Address Filtering: Supports whitelist 

Band Steering (5G Preferred)

WiFi Scheduled Shutdown

User Isolation: Inter-WLAN isolation, AP internal isolation

TX Power Setting

Wireless Client Limit

QoS: WMM

	Network Features
	Connection Type: Static IP, DHCP from server/gateway.

DHCP Server: Built-in or external.

Cloud platform server support.

Firewall.

PPPoE dial-up support.

	Device management
	Configuration backup/restore.

Factory reset.

Reboot (scheduled/instant).

Firmware upgrade.

Time management & synchronization.

System logs.

Fat/Fit AP mode switch.


Interface:
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Dimension:
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Packing:
	AP
	1

	Mounting Accessories
	1


Expertise in ODM wireless communication solutions.

