
WiFi 6 11AX 3000Mbps Outdoor AP
                                                             Model:T300-AX3000
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Description:

T300-AX3000 is a high-performance dual-band 802.11AX product that provides 2.4GHz and 5GHz dual-band wireless services. The 2.4GHz band provides a maximum access rate of 574Mbps, and the 5GHz band provides a maximum access rate of 2402Mbps.

Main Features: 
Dual frequency concurrency, with a maximum wireless concurrency rate of up to 3000Mbps.
IPQ5018 chip greatly expands user capacity and can support 128 users.
Adapted to high gain dual frequency antennas, with a wide coverage range.
The radio frequency uses high-power FEM, with stable performance and longer coverage.
Low power consumption.
Added lightning protection board components, greatly enhancing the protection capability of the equipment.
Hardware Spec:
	Model
	T300-AX3000

	CPU 
	IPQ5018+QCN6102+QCA8337

	Flash
	SPI NOR 8MB，Nand 128MB

	DDR2
	512MB×1

	2.4G Frequency
	2.4GHz ~ 2.484GHz

	2.4G Protocol
	802.11b / g / n / ax

	5G Frequency
	5.150GHz～5.850GHz

	5G Protocol
	802.11a/ n / ac /ax

	Antenna
	4*6dBi Dual Band

	Data Rate
	2.4G 574 Mbps MIMO 2*2, 5G 2402Mbps MIMO 2*2

	2.4G TX Power
	802.11b
	11M
	25±2dBm
	1M
	25±2dBm

	
	802.11g
	54M
	23±2dBm
	6M
	25±2dBm

	
	802.11n HT20
	MCS7
	22±2dBm
	MCS0
	24±2dBm

	
	802.11n HT40
	MCS7
	22±2dBm
	MCS0
	24±2dBm

	
	802.11ax HE20
	MCS11
	20±2dBm
	MCS0
	24±2dBm

	
	802.11ax HE40
	MCS11
	20±2dBm
	MCS0
	24±2dBm

	5G TX Power
	802.11a
	54M
	22±2dBm
	6M
	24±2dBm

	
	802.11n HT20
	MCS7
	21±2dBm
	MCS0
	24±2dBm

	
	802.11n HT40
	MCS7
	21±2dBm
	MCS0
	24±2dBm

	
	802.11ac VHT20
	MCS7
	21±2dBm
	MCS0
	24±2dBm

	
	802.11ac VHT40
	MCS7
	20±2dBm
	MCS0
	24±2dBm

	
	802.11ac VHT80
	MCS9
	20±2dBm
	MCS0
	24±2dBm

	
	802.11ax HE20
	MCS11
	20±2dBm
	MCS0
	24±2dBm

	
	802.11ax HE40
	MCS11
	20±2dBm
	MCS0
	24±2dBm

	
	802.11ax HE80
	MCS11
	19±2dBm
	MCS0
	24±2dBm

	
	802.11ax HE160
	MCS11
	18±2dBm
	MCS0
	23±2dBm

	2.4G Receiving Sensitivity
	802.11b
	11M
	-87dBm
	1M
	-94dBm

	
	802.11g
	54M
	-75dBm
	6M
	-88dBm

	
	802.11n HT20
	MCS7
	-72dBm
	MCS0
	-88dBm

	
	802.11n HT40
	MCS7
	-70dBm
	MCS0
	-88dBm

	
	802.11ax HE20
	MCS11
	-63dBm
	MCS0
	-88dBm

	
	802.11ax HE40
	MCS11
	-61dBm
	MCS0
	-88dBm

	5G Receiving Sensitivity
	802.11a
	54M
	-75dBm
	6M
	-92dBm

	
	802.11n HT20
	MCS7
	-73dBm
	MCS0
	-92dBm

	
	802.11n HT40
	MCS7
	-70dBm
	MCS0
	-90dBm

	
	802.11ac VHT20
	MCS7
	-67dBm
	MCS0
	-88dBm

	
	802.11ac VHT40
	MCS7
	-64dBm
	MCS0
	-88dBm

	
	802.11ac VHT80
	MCS7
	-60dBm
	MCS0
	-88dBm

	
	802.11ax HE20
	MCS11
	-62dBm
	MCS0
	-90dBm

	
	802.11ax HE40
	MCS11
	-60dBm
	MCS0
	-88dBm

	
	802.11ax HE80
	MCS11
	-58dBm
	MCS0
	-86dBm

	
	802.11ax HE160
	MCS11
	-54dBm
	MCS0
	-84dBm

	2.4G EVM
	802.11b: ≤-10 dB ；802.11g: ≤-25 dB ；802.11n: ≤-28dB ;  802.11ax: ≤-35 dB

	5G EVM
	802.11a: ≤-25 dB ；802.11n: ≤-28 dB ；802.11ac: ≤-32 dB;  802.11ax: ≤-35 dB

	ppm
	±20ppm

	WAN
	1*10/100/1000M RJ45, support 48V PoE

	LAN
	1*10/100/1000M LAN

	SFP
	1*10/100/1000M SFP

	POE（WAN）
	802.3at

	Reset
	Reset to factory settings by pressing 6-10 seconds

	Indicators
	WAN, LAN, SYS, 2.4G_WiFi, 5G_WiFi.

	Power
	<18W

	Dimension 
	243.2mm*218.3mm*64.1mm

	Temperature
	Working: -40°C to 70°C；Storage: -40°C to 70°C；Humidity: 5％～95％(Non-Condensing)

	Protection Grade
	IP65

	ESD
	Air:±8K, Touch:±6K

	Electrical Surge
	Common Mode: 4K, Differential Mode: 2K


Firmware Specification:
	Working Mode
	Gateway, AP

	Wireless Functions
	Multiple SSID functions: 2.4GHz: 4; 5.8GHz: 4.

	
	Support SSID hidden 

	
	Support seamless roaming, 802.11kv standard.

	
	Support 5G Prior for a faster Ethernet.

	
	Wireless Security: Open, WPA, WPA2PSK_TKIPAES, WAP2_EAP

	
	Support MAC filter

	
	Support Wi-Fi time on/off to save energy

	
	Support client isolation to improve the wireless stability

	
	Support RF power adjustable, adjust the RF power based on environment.

	
	Support user quantity limited, Max 64 users to access each band.

	Networking Function
	VLAN settings

	
	Cloud access support in gateway mode

	Device Management
	Back-up the configuration

	
	Restore the configuration

	
	Reset to factory default

	
	Reboot the device: including time reboot or reboot immediately

	
	Admin management password modify

	
	Firmware upgrade

	
	System log

	
	Support firmware GUI web management, AC controller management, remote management and cloud management

	Protocols
	IPv4


Interface:
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Packing List:
	AP
	1

	LAN cable
	1

	Installation Accessory
	1



