
11ax 3000Mbps Outdoor Wireless AP 

         Model: T300-AX830-P5
[image: image1.png]



Short Specification

T300-AX830-P5 is a high power and high speed 11ax outdoor wireless AP with Qualcomm chipset.
Support 160MHz bandwidth, the Wi-Fi speed is up to 3000Mbps over 2 radios: 2.4GHz (600Mbps 11ax 2*2) + 5GHz (2400Mbps 2*2), designed in high power FEM and 2.5G WAN and PoE port, omni or directional antenna, it provide 30dBm higher speed and 300meters+ higher range wireless access for users.

Support IP65 waterproof level, light-protection, cloud and APP management, it can be installed at more environment to provide stable wireless coverage.
Main Features:

Wireless data rate up to 3000Mbps 

802.11ax 2x2 MIMO technology, 160MHz bandwidth, the wireless data rate up to 3000Mbps, meet with demand of high-speed applications such as VR/ AR, 4K or 8K stream media.
Power over Ethernet

It is integrated IEEE802.3at Power over Ethernet (PoE), for easy installation and lower cost. So it can be installed in areas where power outlets are not readily available, eliminating the mess of altering existing network infrastructure.

Metal waterproof, dust proof and sunscreen shell, temperature adaptive

With metal waterproof, dust proof and sunscreen shell, avoid the damage from dust, thunderstorm weather. Meantime, it adaptive to various environment, the working temperature can be normal at -20℃ to 55℃. Suit for most environment.
Cloud and APP easy configure and management
Work as FAT AP, it allow users to access and configure it by WEB interface; 

Work as FIT AP, it allow AP controller, cloud or APP remote configure and management; 

Saved a lot maintenance after installation.
Hardware Specification
	Model
	T300-AX830-P5

	CPU 
	IPQ5018 +QCN6102

	Flash
	SPI NOR 8MB

	Nand
	128MB

	DDR3L
	512MB*1

	2.4G Frequency
	2.4GHz – 2.484GHz

	2.4G WIFI Protocol
	802.11 b / g / n /ax

	5G Frequency
	5.150GHz～5.825GHz

	5G WIFI Protocol
	802.11 a / n / ac /ax

	Antenna: 2.4G
	2PCS 2.4G antenna，gain：6dBi

	Antenna: 5G
	2PCS 5.8G antenna，gain：6dBi

	Data Rate
	2.4G: 600Mbps

5G: 2402Mbps

	2.4G RF power
	802.11b
	11M
	26±2dBm
	1M
	26±2dBm

	
	802.11g
	54M
	23±2dBm
	6M
	25±2dBm

	
	802.11n HT20
	MCS7
	22±2dBm
	MCS0
	24±2dBm

	
	802.11n HT40
	MCS7
	22±2dBm
	MCS0
	24±2dBm

	
	802.11ax HE20
	MCS11
	20±2dBm
	MCS0
	24±2dBm

	
	802.11ax HE40
	MCS11
	20±2dBm
	MCS0
	24±2dBm

	5G RF power
	802.11a
	54M
	22±2dBm
	6M
	25±2dBm

	
	802.11n HT20
	MCS7
	21±2dBm
	MCS0
	23±2dBm

	
	802.11n HT40
	MCS7
	21±2dBm
	MCS0
	23±2dBm

	
	802.11ac VHT20
	MCS9
	21±2dBm
	MCS0
	23±2dBm

	
	802.11ac VHT40
	MCS9
	20±2dBm
	MCS0
	23±2dBm

	
	802.11ac VHT80
	MCS9
	20±2dBm
	MCS0
	23±2dBm

	
	802.11ax HE20
	MCS11
	20±2dBm
	MCS0
	22±2dBm

	
	802.11ax HE40
	MCS11
	20±2dBm
	MCS0
	22±2dBm

	
	802.11ax HE80
	MCS11
	20±2dBm
	MCS0
	22±2dBm

	
	802.11ax HE160
	MCS11
	20±2dBm
	MCS0
	22±2dBm

	2.4G Receive Sensitivity
	802.11b
	11M
	-87dBm
	1M
	-94dBm

	
	802.11g
	54M
	-75dBm
	6M
	-88dBm

	
	802.11n HT20
	MCS7
	-72dBm
	MCS0
	-88dBm

	
	802.11n HT40
	MCS7
	-70dBm
	MCS0
	-88dBm

	
	802.11ax HE20
	MCS11
	-63dBm
	MCS0
	-88dBm

	
	802.11ax HE40
	MCS11
	-61dBm
	MCS0
	-88dBm

	5G Receive Sensitivity
	802.11a
	54M
	-75dBm
	6M
	-90dBm

	
	802.11n HT20
	MCS7
	-73dBm
	MCS0
	-88dBm

	
	802.11n HT40
	MCS7
	-63dBm
	MCS0
	-88dBm

	
	802.11ac VHT20
	MCS8
	-67dBm
	MCS0
	-88dBm

	
	802.11ac VHT40
	MCS9
	-64dBm
	MCS0
	-88dBm

	
	802.11ac VHT80
	MCS9
	-60dBm
	MCS0
	-88dBm

	
	802.11ax HE20
	MCS11
	-61dBm
	MCS0
	-88dBm

	
	802.11ax HE40
	MCS11
	-58dBm
	MCS0
	-88dBm

	
	802.11ax HE80
	MCS11
	-55dBm
	MCS0
	-84dBm

	
	802.11ax HE160
	MCS11
	-51dBm
	MCS0
	-82dBm

	2.4G EVM
	802.11b: ≤-10 dB; 802.11g: ≤-25 dB; 802.11n: ≤-28dB;  802.11ax: ≤-35 dB

	5G EVM
	802.11a:≤-25 dB; 802.11n: ≤-28 dB; 802.11ac: ≤-32 dB; 802.11ax: ≤-35 dB

	PPM
	±20ppm

	WAN
	1 * 10/100/1000/2500Mbps WAN port, support 48V POE

	Reset 
	1 * reset button, press 6~10 seconds to restore to factory settings

	Power Supply
	PoE 802.3at

	Maximum power consumption
	< 23W

	Size
	295mm × 231mm × 80mm

	Weight
	2.2kg

	Working Environment
	Normal working temperature:-20°C to 55°C；

Storage temperature:-40°C to 70°C；

Humidity：5％～95％（non-condensing）

	Protection Level
	IP65

	ESD
	By air:  +/-8K，By contact: +/-6K

	Surge
	Common mode: 4KV，Differential mode: 2KV


Firmware Specification

	Working Mode
	Gateway, AP

	Wireless Functions
	Multiple SSID functions: 2.4GHz: 4; 5.8GHz: 4.

	
	Support SSID hidden 

	
	Support seamless roaming, 802.11kvr standard.

	
	Support 5G Prior for a faster Ethernet.

	
	Wireless Security: Open, WPA, WPA2PSK_TKIPAES, WAP2_EAP, 802.1x

	
	Support MAC filter

	
	Support Wi-Fi time on/off to save energy

	
	Support client isolation to improve the wireless stability

	
	Support RF power adjustable, adjust the RF power based on environment.

	
	Support user quantity limited, Max 64 users to access each band.

	Networking Function
	VLAN settings

	
	Cloud access support in gateway mode

	Device Management
	Back-up the configuration

	
	Restore the configuration

	
	Reset to factory default

	
	Reboot the device: including time reboot or reboot immediately

	
	Admin management password modify

	
	Firmware upgrade

	
	System log

	
	Support firmware GUI web management, AC controller management, remote management and cloud management

	Protocols
	IPv4


Product Picture:
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