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Description:
T300-HQ830-P2 is a high-performance 4T4R dual-band 802.11AX product that can provide 2.4G and 5.8GHz dual-band wireless services. 2.4G provides a maximum access rate of 574Mbps, and 5G provides a maximum access rate of 2402Mbps.

Main Features:
· Has better transmission quality, higher transmission rate, and concurrent rate up to 3000Mbps.
· Using IPQ5018 chip, it greatly expands the user capacity and can support 128 users.
· The heat sink adopts snap-on structure design and surface nano-coating treatment, which makes the heat dissipation effect more ideal.
· The radio frequency uses high-power FEM, which has stable performance and farther coverage.
· The addition of lightning protection board components greatly enhances the protection capabilities of the equipment;

Hardware Specification: 
	Model
	[bookmark: _GoBack]T300-HQ830-P2

	CPU 
	IPQ5018 + QCN6102

	Flash
	SPI NOR 8MB  SPI NAND 128MB 

	DDR3
	512MB*1

	2.4G working frequency
	2.4GHz ~ 2.484GHz

	2.4G WIFI protocol
	802.11 b / g / n / ac / ax

	5G working frequency
	5.150GHz～5.825GHz

	5G WIFI protocol
	802.11 a / n / ac / ax

	Internal 2.4G
	2*2.4G: 5dBi

	Internal 5G
	2*5.8G: 7dBi

	Max rate
	2.4G: 574Mbps; 5G: 2402Mbps

	2.4G TX Power
	802.11b
	11M
	24±2dBm
	1M
	24±2dBm

	
	802.11g
	54M
	21±2dBm
	6M
	23±2dBm

	
	802.11n HT20
	MCS7
	20±2dBm
	MCS0
	22±2dBm

	
	802.11n HT40
	MCS7
	20±2dBm
	MCS0
	22±2dBm

	
	802.11ax HE20
	MCS11
	18±2dBm
	MCS0
	22±2dBm

	
	802.11ax HE40
	MCS11
	18±2dBm
	MCS0
	22±2dBm

	5G TX Power
	802.11a
	54M
	19±2dBm
	6M
	22±2dBm

	
	802.11n HT20
	MCS7
	18±2dBm
	MCS0
	21±2dBm

	
	802.11n HT40
	MCS7
	18±2dBm
	MCS0
	21±2dBm

	
	802.11ac VHT20
	MCS9
	17±2dBm
	MCS0
	21±2dBm

	
	802.11ac VHT40
	MCS9
	17±2dBm
	MCS0
	21±2dBm

	
	802.11ac VHT80
	MCS9
	17±2dBm
	MCS0
	21±2dBm

	
	802.11ax HE20
	MCS11
	17±2dBm
	MCS0
	21±2dBm

	
	802.11ax HE40
	MCS11
	17±2dBm
	MCS0
	21±2dBm

	
	802.11ax HE80
	MCS11
	17±2dBm
	MCS0
	21±2dBm

	
	802.11ax HE160
	MCS11
	17±2dBm
	MCS0
	21±2dBm

	2.4G Receiving Sensitivity
	802.11b
	11M
	-85dBm
	1M
	-90dBm

	
	802.11g
	54M
	-72dBm
	6M
	-90dBm

	
	802.11n HT20
	MCS7
	-70dBm
	MCS0
	-87dBm

	
	802.11n HT40
	MCS7
	-68dBm
	MCS0
	-85dBm

	
	802.11ax HE20
	MCS11
	-60dBm
	MCS0
	-83dBm

	
	802.11ax HE40
	MCS11
	-56dBm
	MCS0
	-83dBm

	5G Receiving Sensitivity
	802.11a
	54M
	-72dBm
	6M
	-92dBm

	
	802.11n HT20
	MCS7
	-70dBm
	MCS0
	-90dBm

	
	802.11n HT40
	MCS7
	-68dBm
	MCS0
	-88dBm

	
	802.11ac VHT20
	MCS8
	-70dBm
	MCS0
	-88dBm

	
	802.11ac VHT40
	MCS9
	-68dBm
	MCS0
	-88dBm

	
	802.11ac VHT80
	MCS9
	-58dBm
	MCS0
	-85dBm

	
	802.11ax HE20
	MCS11
	-62dBm
	MCS0
	-88dBm

	
	802.11ax HE40
	MCS11
	-58dBm
	MCS0
	-86dBm

	
	802.11ax HE80
	MCS11
	-55dBm
	MCS0
	-84dBm

	
	802.11ax HE160
	MCS11
	-51dBm
	MCS0
	-82dBm

	2.4G EVM
	802.11b:≤-10 dB ；802.11g: ≤-25 dB ；802.11n:≤-28 dB；802.11ax:≤-35 dB 

	5G EVM
	802.11a:≤-25 dB ；802.11n: ≤-28 dB ；802.11ac:≤-32 dB；802.11ax:≤-35 dB

	ppm
	±20ppm

	WAN
	1*10/100/1000M support 48V POE

	LAN
	1*Console port

	Reset
	Reset to factory settings by pressing 6-10 seconds

	Indicators
	PWR, SYS, WAN, 2.4G, 5.8G

	Power
	PoE 802.3at

	Max Power Consumption
	<16W

	Dimension 
	304mm × 181mm × 88mm

	Weight
	1.6kg

	Temperature
	Working: -20°C to 55°C；Storage: -40°C to 70°C；Humidity: 5％～95％(Non-Condensing)

	IP Grade
	IP67

	ESD
	Air:±8K, Touch:±4K

	Electrical Surge
	Common Mode: 4K, Differential Mode: 2K




Firmware
	Home Page
	Working mode: FIT/ FAT mode

	
	Wireless AP download rate, wireless AP upload rate, runtime

	
	Device information, device description, intranet information, WIFI information

	Working Mode
	Gateway mode: The device connects to the wide area network through a WAN port and then uses static IP, DHCP, or PPPOE to connect to the internet

	
	AP mode: The device covers other clients and devices with wireless network signals, and connects to other routers through Ethernet to access the wide area network

	Wireless feature
	SSID broadcasting

	
	SSID quantity: 4 (2.4GHz)+4()5GHz)

	
	Hide SSID

	
	Wireless encryption: OPEN、WPA/WPA2PSK-TKIPAES、WPA3PSK-TKIPAES

	
	MAC filter

	
	Band steering (5G WiFi priority)

	
	WiFi timed shutdown

	
	User isolation: wireless network isolation, AP internal isolation

	
	TX power adjustable

	
	Wireless client quantity limit

	
	QoS: WMM

	Network feature
Cloud Platform Server
	Connection method: static address, obtained from management server, obtained from gateway

	
	DHCP server: It can be either a built-in DHCP server or an external DHCP server

	
	Cloud Platform Server support

	
	Firewall

	
	PPPOE

	Device management
	Backup

	
	Recovery

	
	Reset to factory

	
	Timed reboot/ Instant reboot

	
	Firmware upgrade

	
	System log

	
	FIT/ FAT AP switch



Interface
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Dimension
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Accessory
	AP
	1

	Mounting Accessories
	2

	Gift Box
	1
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