
WiFi 7 3600Mbps Inwall Wireless AP 

                   Model: T300-FAP836
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Short Specification

T300-FAP836 is a high-performance, high-speed indoor Wi-Fi 7 panel AP, delivering dual-band wireless services (2.4GHz and 5GHz) for a fast and stable wireless connectivity experience.

Main Features:

Compliant with IEEE 802.11be (Wi-Fi 7), supporting MLO and 4096QAM.

Maximum wireless speeds of up to 3570Mbps (2.4GHz: 688Mbps + 5GHz: 2882Mbps).

Uplink 2.5Gbps Ethernet port, downlink Gigabit Ethernet port.

Supports standard PoE power supply, compliant with IEEE 802.3at.

Hardware watchdog function for automatic device recovery in case of anomalies, maintenance-free.

Metal base casing for superior heat dissipation.

Hardware Specification
	Model
	T300-FAP836

	CPU 
	AN7563+MT7991B+MT7976CN+EN8811H

	Flash
	NAND 128MB

	DDR3
	512MB

	2.4G Frequency
	2.4GHz – 2.4835GHz

	2.4G Protocol
	802.11 b / g / n / ax / be

	5G Frequency
	5.150GHz～5.850GHz

	5G Protocol
	802.11 a / n / ac / ax / be

	Antenna
	2*dual band antenna: 2.4G 1.7dBi; 5G 3dBi

	Data Rate
	5G: 2402Mbps   2.4G:574Mbps

	2.4G TX Power
	802.11b
	11M
	23±2dBm
	1M
	23±2dBm

	
	802.11g
	54M
	20±2dBm
	6M
	22±2dBm

	
	802.11n HT20
	MCS7
	18.5±2dBm
	MCS0
	20.5±2dBm

	
	802.11n HT40
	MCS7
	18.5±2dBm
	MCS0
	20.5±2dBm

	
	802.11ax HE20
	MCS11
	17±2dBm
	MCS0
	20.5±2dBm

	
	802.11ax HE40
	MCS11
	17±2dBm
	MCS0
	20.5±2dBm

	
	802.11be EHT20
	MCS13
	16±2dBm
	MCS0
	20.5±2dBm

	
	802.11be EHT40
	MCS13
	16±2dBm
	MCS0
	20.5±2dBm

	5G TX Power
	802.11a
	54M
	19.5±2dBm
	6M
	22±2dBm

	
	802.11n HT20
	MCS7
	19±2dBm
	MCS0
	21±2dBm

	
	802.11n HT40
	MCS7
	19±2dBm
	MCS0
	21±2dBm

	
	802.11ac VHT20
	MCS7
	18.5±2dBm
	MCS0
	21±2dBm

	
	802.11ac VHT40
	MCS7
	18.5±2dBm
	MCS0
	20.5±2dBm

	
	802.11ac VHT80
	MCS9
	18.5±2dBm
	MCS0
	20.5±2dBm

	
	802.11ax HE20
	MCS11
	18±2dBm
	MCS0
	21±2dBm

	
	802.11ax HE40
	MCS11
	18±2dBm
	MCS0
	20.5±2dBm

	
	802.11ax HE80
	MCS11
	17±2dBm
	MCS0
	20.5±2dBm

	
	802.11ax HE160
	MCS11
	16±2dBm
	MCS0
	19.5±2dBm

	
	802.11be EHT20
	MCS13
	16.5±2dBm
	MCS0
	21±2dBm

	
	802.11be EHT40
	MCS13
	16±2dBm
	MCS0
	20.5±2dBm

	
	802.11be EHT80
	MCS13
	15.5±2dBm
	MCS0
	20.5±2dBm

	
	802.11be EHT160
	MCS13
	14.5±2dBm
	MCS0
	19.5±2dBm

	2.4G Receiving Sensitivity
	802.11b
	11M
	-87dBm
	1M
	-95dBm

	
	802.11g
	54M
	-75dBm
	6M
	-92dBm

	
	802.11n HT20
	MCS7
	-74dBm
	MCS0
	-92dBm

	
	802.11n HT40
	MCS7
	-71dBm
	MCS0
	-89dBm

	
	802.11ax HE20
	MCS11
	-63dBm
	MCS0
	-92dBm

	
	802.11ax HE40
	MCS11
	-60dBm
	MCS0
	-88dBm

	
	802.11be EHT20
	MCS13
	-56dBm
	MCS0
	-92dBm

	
	802.11be EHT40
	MCS13
	-53dBm
	MCS0
	-89dBm

	5G Receiving Sensitivity
	802.11a
	54M
	-74dBm
	6M
	-91dBm

	
	802.11n HT20
	MCS7
	-73dBm
	MCS0 
	-90dBm

	
	802.11n HT40
	MCS7
	-70dBm
	MCS0 
	-87dBm

	
	802.11ac VHT20
	MCS7
	-67dBm
	MCS0 
	-91dBm

	
	802.11ac VHT40
	MCS7
	-63dBm
	MCS0
	-88dBm

	
	802.11ac VHT80
	MCS9
	-60dBm
	MCS0
	-85dBm

	
	802.11ax HE20
	MCS11
	-62dBm
	MCS0
	-91dBm

	
	802.11ax HE40
	MCS11
	-59dBm
	MCS0
	-89dBm

	
	802.11ax HE80
	MCS11
	-56dBm
	MCS0
	-86dBm

	
	802.11ax HE160
	MCS11
	-53dBm
	MCS0
	-83dBm

	
	802.11be EHT20
	MCS13
	-55dBm
	MCS0
	-91dBm

	
	802.11be EHT40
	MCS13
	-52dBm
	MCS0
	-88dBm

	
	802.11be EHT80
	MCS13
	-49dBm
	MCS0
	-85dBm

	
	802.11be EHT160
	MCS13
	-46dBm
	MCS0
	-82dBm

	2.4G EVM
	802.11b: ≤-10 dB；802.11g: ≤-25 dB；802.11n: ≤-28dB；

802.11ax: ≤-35 dB；802.11be: ≤-38 dB 

	5G EVM
	802.11a: ≤-25 dB；802.11n: ≤-28 dB；802.11ac: ≤-32 dB；

802.11ax: ≤-35 dB；802.11be: ≤-38 dB

	ppm
	±20ppm

	WAN
	1*10/1000/2500M WAN, support PoE 48V

	LAN
	1*10/100/1000M LAN


POE

	 
	802.3at

	Reset
	Reset to factory settings by pressing 6-10 seconds

	Indicators
	SYS

	Max Power Consumption
	<14W

	ESD
	Air:±8K, Touch:±6K

	Electrical Surge
	Common Mode: 2K, Differential Mode: 1K

	Size
	86mm*86mm*42.8mm(10.8mm beyond the wall)                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     

	Weight
	0.22kg

	Temperature
	Working: -10°C to 40°C；Storage: -40°C to 70°C；Humidity: 5％～95％(Non-Condensing)


Firmware Specification

	Working Mode
	AP (FAT/FIT)

	Wireless Functions
	Multiple SSID functions: 2.4GHz: 4; 5.8GHz: 4.

	
	Support SSID hidden 

	
	Support seamless roaming

	
	Support 5G Prior for a faster Ethernet.

	
	Wireless Security: OPEN, WPA/WPA2PSK-TKIPAES, WPA2PSK-TKIPAES, WPA3PSK-AES

	
	Support MAC filter

	
	Support Wi-Fi time on/off to save energy

	
	Support client isolation to improve the wireless stability

	
	Support RF power adjustable, adjust the RF power based on environment.

	Networking Function
	VLAN settings

	
	Cloud access support in gateway mode

	Device Management
	Back-up the configuration

	
	Restore the configuration

	
	Reset to factory default

	
	Reboot the device: including time reboot or reboot immediately

	
	Admin management password modify

	
	Firmware upgrade

	
	System log

	
	Support firmware GUI web management, AC controller management, remote management and cloud management

	Protocols
	IPv4


Interface
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Dimension

[image: image3.png]sE

=

| —

D)

Ya
QO

86

)

473 =0

66,9





Packing List
	AP
	1

	Screw
	2



